Figure S01: Domain photo with evaluation points in Delnicka street. Photo provided by The Prague Institute of Planning and Development.
Figure S02: Domain photo with evaluation points in Komunardu street. Photo provided by The Prague Institute of Planning and Development.
Figure S03: Domain photo with evaluation points in courtyards and the main crossroad. Photo provided by The Prague Institute of Planning and Development.
Figure S04: Main crossroad photo with evaluation points. Photo provided by The Prague Institute of Planning and Development.
Figure S05: Domain photo; red-shaded area shows placement of all gridboxes used for averaging over the entire domain. Photo provided by The Prague Institute of Planning and Development.
Figure S06: Domain photo; red-shaded area shows placement of gridboxes used for averaging in Delnicka street. Photo provided by The Prague Institute of Planning and Development.
Figure S07: Domain photo; red-shaded area shows placement of gridboxes used for averaging in Komunardu street. Photo provided by The Prague Institute of Planning and Development.
Figure S08: Domain photo; red-shaded area shows placement of gridboxes used for averaging in courtyards only. Photo provided by The Prague Institute of Planning and Development.
Figure S09: Domain photo; red-shaded area shows placement of gridboxes used for averaging in streets only. Photo provided by The Prague Institute of Planning and Development.
Figure S10: PM2.5 emitted by the cars along their trajectories in Prague-Holešovice.\nConcentrations were summarized in g.day-1.m-2 and disaggregated to 1-hour time steps.\nOrthophoto source: Institute of Prague Development.
Figure S11: Sensitivity (scenario-baseline) of 24-hour average surface temperature in SA (left) and SB (right) scenarios.\nBox colors indicate related scenarios (e.g., blue: changing albedo, orange: changing emissivity, etc.)
Figure S12: Sensitivity (scenario-baseline) of 24-hour average MRT (mean radiant temperature) in SA (left) and SB (right) scenarios.\nBox colors indicate related scenarios (e.g., blue: changing albedo, orange: changing emissivity, etc.)
Figure S13: Sensitivity (scenario-baseline) of 24-hour average PET (mean radiant temperature) in SA (left) and SB (right) scenarios.\nBox colors indicate related scenarios (e.g., blue: changing albedo, orange: changing emissivity, etc.)
Figure S14: Sensitivity (scenario-baseline) of 24-hour average PM2.5 concentrations (mean radiant temperature) in SA (left) and SB (right) scenarios.\nBox colors indicate related scenarios (e.g., blue: changing albedo, orange: changing emissivity, etc.)
Figure S15: Net radiation at points A01 (PA01, solid) and A02 (PA02, dashed)\nin scenarios with increased (blue) and decreased (orange) albedo compared to the baseline (black).
