 
 Starting EDDA 1.5     15 June 201
 Date 03/14/2017
 Time 11:05:53
 initialization file -->
 edda_in.txt                                                                    
                                                                                
                                                                                
                   
 -- LISTING OF INITIALIZATION FILE --
 EDDA: integrated simulation of debris flow erosion, deposition and property cha
 nges (up to 255 characters)                                                    
                                                                                
                   
 EDDA_1.5                                                                       
                                                                                
                                                                                
                   
 imax, row, col, nwf, tx, nmax,flow-direction numbering scheme (ESRI=1, TopoInde
 x=2)                                                                           
                                                                                
                   
        9595         158         111      200000           1          10
           1
 nzsb, nzst, mmax, nper,  zmin,  uww,     t(rainfall), zones                    
                                                                                
                                                                                
                   
          26          26         100          46  1.000000000000000E-003
   9800.00000000000        165600.000000000                4
 ltstar, lbstar, zmax,   depth,   rizero,  Min_Slope_Angle (degrees)            
                                                                                
                                                                                
                   
  -3.00000000000000        4.00000000000000        7.00000000000000     
   7.00000000000000       1.000000000000000E-009  0.100000000000000     
 nsection                                                                       
                                                                                
                                                                                
                   
          18
 zone:            1
 cohesion,sdcohesion,phi, sdphi,phib, sdphib,uws,   diffus,   K-sat, Theta-sat,T
 heta-res,Theta-ini,porosity, psi, Alpha (bottom layer)                         
                                                                                
                   
   10500.0000000000        5250.00000000000        37.0000000000000     
   5.55000000000000        24.6000000000000        3.69000000000000     
   21000.0000000000       2.300000000000000E-005  1.000000000000000E-006
  0.400000000000000       0.250000000000000       0.115500000000000     
  0.350000000000000       5.100000000000000E-002  0.800000000000000     
 cohesion,sdcohesion,phi, sdphi,phib, sdphib,uws,   diffus,   K-sat, Theta-sat,T
 heta-res,Theta-ini,porosity, psi, Alpha, kero (top layer)                      
                                                                                
                   
   10500.0000000000        5250.00000000000        37.0000000000000     
   5.55000000000000        24.6000000000000        3.69000000000000     
   21000.0000000000       2.300000000000000E-005  1.000000000000000E-006
  0.400000000000000       0.250000000000000       0.115500000000000     
  0.350000000000000       5.100000000000000E-002  0.800000000000000     
  0.000000000000000E+000
 Unsaturated infiltration model will be used for cells in zone           1 .
 zone:            2
 cohesion,sdcohesion,phi, sdphi,phib, sdphib,uws,   diffus,   K-sat, Theta-sat,T
 heta-res,Theta-ini,porosity, psi, Alpha (bottom layer)                         
                                                                                
                   
   20000000.0000000        1000.00000000000        5.00000000000000     
  0.750000000000000        3.50000000000000       0.530000000000000     
   27000.0000000000       5.000000000000000E-013  1.000000000000000E-013
  1.000000000000000E-003  5.000000000000000E-004  3.000000000000000E-004
  1.000000000000000E-003  5.100000000000000E-002  0.500000000000000     
 cohesion,sdcohesion,phi, sdphi,phib, sdphib,uws,   diffus,   K-sat, Theta-sat,T
 heta-res,Theta-ini,porosity, psi, Alpha, kero (top layer)                      
                                                                                
                   
   20000000.0000000        1000.00000000000        5.00000000000000     
  0.750000000000000        3.50000000000000       0.530000000000000     
   27000.0000000000       5.000000000000000E-013  1.000000000000000E-013
  1.000000000000000E-003  5.000000000000000E-004  3.000000000000000E-004
  1.000000000000000E-003  5.100000000000000E-002  0.500000000000000     
  0.000000000000000E+000
 Unsaturated infiltration model will be used for cells in zone           2 .
 zone:            3
 cohesion,sdcohesion,phi, sdphi,phib, sdphib,uws,   diffus,   K-sat, Theta-sat,T
 heta-res,Theta-ini,porosity, psi, Alpha (bottom layer)                         
                                                                                
                   
   10500.0000000000        5250.00000000000        37.0000000000000     
   5.55000000000000        24.6000000000000        3.69000000000000     
   21000.0000000000       2.300000000000000E-005  1.000000000000000E-006
  0.400000000000000       0.250000000000000       0.115500000000000     
  0.510000000000000       5.100000000000000E-002  0.800000000000000     
 cohesion,sdcohesion,phi, sdphi,phib, sdphib,uws,   diffus,   K-sat, Theta-sat,T
 heta-res,Theta-ini,porosity, psi, Alpha, kero (top layer)                      
                                                                                
                   
   4000.00000000000        2000.00000000000        37.0000000000000     
   5.55000000000000        24.6000000000000        3.69000000000000     
   21000.0000000000       2.300000000000000E-005  1.000000000000000E-005
  0.420000000000000       0.180000000000000       0.115500000000000     
  0.510000000000000       5.100000000000000E-002  0.800000000000000     
  7.849999999999999E-008
 Unsaturated infiltration model will be used for cells in zone           3 .
 zone:            4
 cohesion,sdcohesion,phi, sdphi,phib, sdphib,uws,   diffus,   K-sat, Theta-sat,T
 heta-res,Theta-ini,porosity, psi, Alpha (bottom layer)                         
                                                                                
                   
   20000000.0000000        1000.00000000000        34.0000000000000     
   5.10000000000000        20.0000000000000        3.00000000000000     
   21000.0000000000       5.000000000000000E-006  1.000000000000000E-003
  0.350000000000000       5.000000000000000E-002  0.115500000000000     
  0.350000000000000       5.100000000000000E-002   1.00000000000000     
 cohesion,sdcohesion,phi, sdphi,phib, sdphib,uws,   diffus,   K-sat, Theta-sat,T
 heta-res,Theta-ini,porosity, psi, Alpha, kero (top layer)                      
                                                                                
                   
   20000000.0000000        1000.00000000000        34.0000000000000     
   5.10000000000000        20.0000000000000        3.00000000000000     
   21000.0000000000       5.000000000000000E-006  1.000000000000000E-003
  0.350000000000000       5.000000000000000E-002  0.115500000000000     
  0.350000000000000       5.100000000000000E-002   1.00000000000000     
  0.000000000000000E+000
 Unsaturated infiltration model will be used for cells in zone           4 .
 cri(1), cri(2), ..., cri(nper)                                                 
                                                                                
                                                                                
                   
  2.100000000000000E-006  0.000000000000000E+000  0.000000000000000E+000
  0.000000000000000E+000  0.000000000000000E+000  0.000000000000000E+000
  3.300000000000000E-006  9.700000000000000E-007  1.100000000000000E-006
  5.600000000000000E-008  2.800000000000000E-008  5.600000000000000E-008
  0.000000000000000E+000  3.000000000000000E-006  8.899999999999999E-006
  2.500000000000000E-007  2.200000000000000E-007  2.800000000000000E-008
  0.000000000000000E+000  0.000000000000000E+000  0.000000000000000E+000
  0.000000000000000E+000  0.000000000000000E+000  0.000000000000000E+000
  0.000000000000000E+000  0.000000000000000E+000  0.000000000000000E+000
  7.800000000000000E-007  0.000000000000000E+000  1.100000000000000E-007
  1.800000000000000E-006  1.800000000000000E-006  1.700000000000000E-006
  4.900000000000000E-006  3.400000000000000E-006  6.100000000000000E-006
  4.600000000000000E-006  9.400000000000000E-007  2.800000000000000E-007
  6.700000000000000E-007  4.600000000000000E-006  2.700000000000000E-006
  6.100000000000000E-006  2.000000000000000E-006  5.600000000000000E-007
  2.800000000000000E-008
 capt(1), capt(2), ..., capt(n), capt(n+1)                                      
                                                                                
                                                                                
                   
  0.000000000000000E+000   3600.00000000000        7200.00000000000     
   10800.0000000000        14400.0000000000        18000.0000000000     
   21600.0000000000        25200.0000000000        28800.0000000000     
   32400.0000000000        36000.0000000000        39600.0000000000     
   43200.0000000000        46800.0000000000        50400.0000000000     
   54000.0000000000        57600.0000000000        61200.0000000000     
   64800.0000000000        68400.0000000000        72000.0000000000     
   75600.0000000000        79200.0000000000        82800.0000000000     
   86400.0000000000        90000.0000000000        93600.0000000000     
   97200.0000000000        100800.000000000        104400.000000000     
   108000.000000000        111600.000000000        115200.000000000     
   118800.000000000        122400.000000000        126000.000000000     
   129600.000000000        133200.000000000        136800.000000000     
   140400.000000000        144000.000000000        147600.000000000     
   151200.000000000        154800.000000000        158400.000000000     
   162000.000000000        165600.000000000     
 File name of slope angle grid (slofil)                                         
                                                                                
                                                                                
                   
 Data\tutorial\slope.asc                                                        
                                                                                
                                                                                
                   
 File name of dem file grid (demfil)                                            
                                                                                
                                                                                
                   
 Data\tutorial\dem.asc                                                          
                                                                                
                                                                                
                   
 File name of manning coefficients (manningfil)                                 
                                                                                
                                                                                
                   
 Data\tutorial\manning.asc                                                      
                                                                                
                                                                                
                   
 File name of direction grid (dirfil)                                           
                                                                                
                                                                                
                   
 data\tutorial\directions.asc                                                   
                                                                                
                                                                                
                   
 File name of property zone grid (zonfil)                                       
                                                                                
                                                                                
                   
 Data\tutorial\zones.asc                                                        
                                                                                
                                                                                
                   
 File name of depth grid (zfil)                                                 
                                                                                
                                                                                
                   
 Data\tutorial\ltstar.asc                                                       
                                                                                
                                                                                
                   
 File name of initial depth of water table grid   (depfil)                      
                                                                                
                                                                                
                   
 Data\tutorial\depthwt.asc                                                      
                                                                                
                                                                                
                   
 File name of initial infiltration rate grid   (rizerofil)                      
                                                                                
                                                                                
                   
 Data\tutorial\rizero.asc                                                       
                                                                                
                                                                                
                   
 File name of road map grid   (roadfil)                                         
                                                                                
                                                                                
                   
 Data\tutorial\road.asc                                                         
                                                                                
                                                                                
                   
 File name of catchment grid   (catchmentfil)                                   
                                                                                
                                                                                
                   
 Data\tutorial\catchment.asc                                                    
                                                                                
                                                                                
                   
 File name of mouthpoint grid   (mouthpointfil)                                 
                                                                                
                                                                                
                   
 Data\tutorial\mouthpoint.asc                                                   
                                                                                
                                                                                
                   
 List of file name(s) of rainfall intensity for each period, (rifil())          
                                                                                
                                                                                
                   
 Data\tutorial\ri1.txt                                                          
                                                                                
                                                                                
                   
 Data\tutorial\ri2.txt                                                          
                                                                                
                                                                                
                   
 Data\tutorial\ri3.txt                                                          
                                                                                
                                                                                
                   
 Data\tutorial\ri4.txt                                                          
                                                                                
                                                                                
                   
 Data\tutorial\ri5.txt                                                          
                                                                                
                                                                                
                   
 Data\tutorial\ri6.txt                                                          
                                                                                
                                                                                
                   
 Data\tutorial\ri7.txt                                                          
                                                                                
                                                                                
                   
 Data\tutorial\ri8.txt                                                          
                                                                                
                                                                                
                   
 Data\tutorial\ri9.txt                                                          
                                                                                
                                                                                
                   
 Data\tutorial\ri10.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri11.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri12.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri13.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri14.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri15.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri16.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri17.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri18.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri19.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri20.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri21.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri22.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri23.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri24.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri25.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri26.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri27.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri28.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri29.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri30.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri31.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri32.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri33.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri34.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri35.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri36.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri37.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri38.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri39.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri40.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri41.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri42.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri43.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri44.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri45.txt                                                         
                                                                                
                                                                                
                   
 Data\tutorial\ri46.txt                                                         
                                                                                
                                                                                
                   
 File name of grid of D8 runoff receptor cell numbers (nxtfil)                  
                                                                                
                                                                                
                   
 Data\topo\TIdscelGrid_tutorial.txt                                             
                                                                                
                                                                                
                   
 File name of list of defining runoff computation order (ndxfil)                
                                                                                
                                                                                
                   
 Data\topo\TIcelindxList_tutorial.txt                                           
                                                                                
                                                                                
                   
 File name of list of all runoff receptor cells  (dscfil)                       
                                                                                
                                                                                
                   
 Data\topo\TIdscelList_tutorial.txt                                             
                                                                                
                                                                                
                   
 File name of list of runoff weighting factors  (wffil)                         
                                                                                
                                                                                
                   
 Data\topo\TIwfactorList_tutorial.txt                                           
                                                                                
                                                                                
                   
 Folder where output grid files will be stored  (folder)                        
                                                                                
                                                                                
                   
 results\                                                                       
                                                                                
                                                                                
                   
 Identification code to be added to names of output files (suffix)              
                                                                                
                                                                                
                   
 EDDA    
 Save grid files of runoff? Enter T (.true.) or F (.false.)                     
                                                                                
                                                                                
                   
 F
 Save grid of minimum factor of safety? Enter Enter T (.true.) or F (.false.)   
                                                                                
                                                                                
                   
 T
 Save grid of depth of minimum factor of safety? Enter Enter T (.true.) or F (.f
 alse.)                                                                         
                                                                                
                   
 F
 Save grid of pore pressure at depth of minimum factor of safety? Enter Enter T 
 (.true.) or F (.false.)                                                        
                                                                                
                   
 F
 Save grid files of actual infiltration rate? Enter T (.true.) or F (.false.)   
                                                                                
                                                                                
                   
 F
 Save grid files of unsaturated zone basal flux? Enter T (.true.) or F (.false.)
                                                                                
                                                                                
                   
 F
 Save grid files of the deposit distribution? Enter T (.true.) or F (.false.)   
                                                                                
                                                                                
                   
 T
 Save grid of probability of failure (pf) at depth of minimum factor of safety? 
 Enter Enter T (.true.) or F (.false.)                                          
                                                                                
                   
 T
 Save grid of risk imposed by the slope failure to the road? Enter Enter T (.tru
 e.) or F (.false.)                                                             
                                                                                
                   
 F
 Save grid of warning level along the road? Enter Enter T (.true.) or F (.false.
 )                                                                              
                                                                                
                   
 T
 Save grid of trace of the detached material and debris? Enter Enter T (.true.) 
 or F (.false.)                                                                 
                                                                                
                   
 T
 Save listing of pressure head and factor of safety ("flag")? (Enter -2 detailed
 , -1 normal, 0 none)                                                           
                                                                                
                   
          -1
 Number of times to save output grids of slope failures                         
                                                                                
                                                                                
                   
           1
 Times of output grids                                                          
                                                                                
                                                                                
                   
   3600.00000000000     
 Skip other timesteps? Enter T (.true.) or F (.false.)                          
                                                                                
                                                                                
                   
 F
 Use analytic solution for fillable porosity?  Enter T (.true.) or F (.false.)  
                                                                                
                                                                                
                   
 T
 Estimate positive pressure head in rising water table zone (i.e. in lower part 
 of unsat zone)?  Enter T (.true.) or F (.false.)                               
                                                                                
                   
 T
 Use psi0=-1/alpha? Enter T (.true.) or F (.false.) (False selects the default v
 alue, psi0=0)                                                                  
                                                                                
                   
 F
 Log mass balance results?   Enter T (.true.) or F (.false.)                    
                                                                                
                                                                                
                   
 T
 Flow direction (enter "gener", "slope", or "hydro")                            
                                                                                
                                                                                
                   
 slope
 Add steady background flux to transient infiltration rate to prevent drying bey
 ond the initial conditions during periods of zero infiltration?                
                                                                                
                   
 T
 Initiaion information for Whole processes of Debris flow simulation            
                                                                                
                                                                                
                   
 alpha1 beta1 alpha2   beta2   K     manning  limitfr  shallown                 
                                                                                
                                                                                
                   
   3.80000000000000        3.51000000000000       2.000000000000000E-002
   2.97000000000000        2500.00000000000       0.160000000000000     
   1.00000000000000       0.200000000000000     
 d50    cvstar  coedepo  cs                                                     
                                                                                
                                                                                
                   
  3.500000000000000E-002  0.650000000000000       2.000000000000000E-002
  0.500000000000000     
 dtmin(s)   dtmax(s)   dti(s)   dtd(s)   simul(s)  tout(s)   toldh(m)   toldhp  
 wavemax                                                                        
                                                                                
                   
  1.000000000000000E-005   1.00000000000000       1.000000000000000E-004
  1.000000000000000E-003   165600.000000000        180.000000000000     
  5.000000000000000E-002  0.200000000000000       0.250000000000000     
 Using the full dynamic wave equation to compute the velocity?  T using full dyn
 amic wave equation, F using diffusive wave equation                            
                                                                                
                   
 T
 Simulte rainfall? Enter T (.true.) or F (.false.)                              
                                                                                
                                                                                
                   
 T
 Simulte infiltration? Enter T (.true.) or F (.false.)                          
                                                                                
                                                                                
                   
 T
 Simulate inflow hydrograph? Enter T (.true.) or F (.false.)                    
                                                                                
                                                                                
                   
 F
 Simulate outflow cell? Enter T (.true.) or F (.false.)                         
                                                                                
                                                                                
                   
 T
 Simulate shallow landslide? Enter T (.true.) or F (.false.)                    
                                                                                
                                                                                
                   
 T
 Simulate debris flow? Enter T (.true.) or F (.false.)                          
                                                                                
                                                                                
                   
 T
 Simulte erosion? Enter T (.true.) or F (.false.)                               
                                                                                
                                                                                
                   
 T
 Simulte simulate the water and solid material seperately? Enter T (.true.) or F
  (.false.)                                                                     
                                                                                
                   
 T
 Save grid of minimum factor of safety? Enter T (.true.) or F (.false.)         
                                                                                
                                                                                
                   
 T
 Save grid of flow depth? Enter T (.true.) or F (.false.)                       
                                                                                
                                                                                
                   
 T
 Save grid of maximum flow depth? Enter T (.true.) or F (.false.)               
                                                                                
                                                                                
                   
 T
 Save grid of flow velocity? Enter T (.true.) or F (.false.)                    
                                                                                
                                                                                
                   
 T
 Save grid of maximum flow velocity? Enter T (.true.) or F (.false.)            
                                                                                
                                                                                
                   
 T
 Save grid of Erosion depth? Enter T (.true.) or F (.false.)                    
                                                                                
                                                                                
                   
 T
 Save grid of deposition depth when simulating water and soil deposition seperat
 ely? Enter T (.true.) or F (.false.)                                           
                                                                                
                   
 T
 Save grid of total depth of flow depth and deposit depth? Enter T (.true.) or F
  (.false.)                                                                     
                                                                                
                   
 T
 Save grid of volumetric sediment concentration? Enter T (.true.) or F (.false.)
                                                                                
                                                                                
                   
 T
 Save outflow process? Enter T (.true.) or F (.false.)                          
                                                                                
                                                                                
                   
 T
 Save hydrograph of specified cells? Enter T (.true.) or F (.false.)            
                                                                                
                                                                                
                   
 T
 -- END OF INITIALIZATION DATA --
 
 EDDA_1.5                                                                       
                                                                                
                                                                                
                   
 
 ******** Zone            1  *********
 Using unsaturated infiltration model.
 Cells where water table is shallower than 
               1.25000000000000     
 treated as tension saturated--Saturated infiltration model used.
 ******** Zone            2  *********
 Using unsaturated infiltration model.
 Cells where water table is shallower than 
               2.00000000000000     
 treated as tension saturated--Saturated infiltration model used.
 ******** Zone            3  *********
 Using unsaturated infiltration model.
 Cells where water table is shallower than 
               1.25000000000000     
 treated as tension saturated--Saturated infiltration model used.
 ******** Zone            4  *********
 Using unsaturated infiltration model.
 Cells where water table is shallower than 
               1.00000000000000     
 treated as tension saturated--Saturated infiltration model used.
 Input file name,            Cell count
 Dem file  grid
 Data\tutorial\dem.asc        9595  data cells
 Slope file  grid
 Data\tutorial\slope.asc        9595  data cells
 Upper layer soil thickness file  grid
 Data\tutorial\ltstar.asc        9595  data cells
 Property zone grid
 Data\tutorial\zones.asc        9595  data cells
 outflow cell file -->
 outflow.txt                                                                    
                                                                                
                                                                                
                   
 -- LISTING OF OUTFLOW CELL FILE --
 Number of outflow cells (i.e. number of cells applied outflow hydrograph)      
                                                                                
                                                                                
                   
          11
        8716
        8745
        8776
        8808
        8841
        8876
        8913
        8952
        8992
        9034
        9078
 Read the outflow cell successfully!
 hydrograph cell file -->
 hydrograph.txt                                                                 
                                                                                
                                                                                
                   
 -- LISTING OF HYDROGRAPH CELL FILE --
 Number of hydrograph cells (i.e. number of cells to be recorded its hydrograph)
                                                                                
                                                                                
                   
          41
        5963
        5964
        6035
        6036
        6107
        6108
        6452
        6453
        6519
        6520
        6521
        6586
        6587
        6904
        6905
        6906
        6966
        6967
        6968
        6790
        6791
        6853
        6854
        6914
        7151
        7152
        7209
        7210
        7267
        7543
        7544
        7545
        7598
        7599
        7600
        7653
        7654
        7655
        7708
        7762
        7763
 Read the hydrograph cell successfully!
 ---------------******---------------
 Adjusted steady infiltration rate, cell         4599
 Corrected rizero/Kst =   0.769329301885975     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4600
 Corrected rizero/Kst =   0.829275236084934     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4601
 Corrected rizero/Kst =   0.833241561197396     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4602
 Corrected rizero/Kst =   0.834754551560094     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4603
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4604
 Corrected rizero/Kst =   0.747615194835508     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4605
 Corrected rizero/Kst =   0.668780186227450     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4606
 Corrected rizero/Kst =   0.668780186227450     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4607
 Corrected rizero/Kst =   0.720619470514862     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4608
 Corrected rizero/Kst =   0.774988047251346     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4680
 Corrected rizero/Kst =   0.795199880745011     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4681
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4682
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4683
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4684
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4685
 Corrected rizero/Kst =   0.747615194835508     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4686
 Corrected rizero/Kst =   0.668780186227450     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4687
 Corrected rizero/Kst =   0.668780186227450     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4688
 Corrected rizero/Kst =   0.730387850649264     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4689
 Corrected rizero/Kst =   0.794466126089298     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4690
 Corrected rizero/Kst =   0.794050756773443     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4760
 Corrected rizero/Kst =   0.833306018101803     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4761
 Corrected rizero/Kst =   0.819094167959211     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4762
 Corrected rizero/Kst =   0.829275236084934     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4763
 Corrected rizero/Kst =   0.833241561197396     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4764
 Corrected rizero/Kst =   0.834754551560094     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4765
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4766
 Corrected rizero/Kst =   0.747615194835508     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4767
 Corrected rizero/Kst =   0.668780186227450     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4768
 Corrected rizero/Kst =   0.668780186227450     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4769
 Corrected rizero/Kst =   0.740960839877007     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4770
 Corrected rizero/Kst =   0.817225265067168     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4771
 Corrected rizero/Kst =   0.823470406692300     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4772
 Corrected rizero/Kst =   0.843738515461640     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4773
 Corrected rizero/Kst =   0.844785106273586     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4841
 Corrected rizero/Kst =   0.832415841648773     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4842
 Corrected rizero/Kst =   0.817225265067168     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4843
 Corrected rizero/Kst =   0.823470406692300     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4844
 Corrected rizero/Kst =   0.843738515461640     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4845
 Corrected rizero/Kst =   0.844785106273586     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4846
 Corrected rizero/Kst =   0.747615194835508     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4847
 Corrected rizero/Kst =   0.668780186227450     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4848
 Corrected rizero/Kst =   0.668780186227450     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4849
 Corrected rizero/Kst =   0.746376178951104     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4850
 Corrected rizero/Kst =   0.829275236084934     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4851
 Corrected rizero/Kst =   0.833241561197396     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4852
 Corrected rizero/Kst =   0.834754551560094     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4853
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4854
 Corrected rizero/Kst =   0.747615194835508     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4922
 Corrected rizero/Kst =   0.823928119121235     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4923
 Corrected rizero/Kst =   0.806482983676089     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4924
 Corrected rizero/Kst =   0.793954947555435     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4925
 Corrected rizero/Kst =   0.820827633236507     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4926
 Corrected rizero/Kst =   0.812439830294237     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4927
 Corrected rizero/Kst =   0.743816419745419     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4928
 Corrected rizero/Kst =   0.692916850817795     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4929
 Corrected rizero/Kst =   0.679160402043108     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4930
 Corrected rizero/Kst =   0.753608467723462     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4931
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4932
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4933
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4934
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         4935
 Corrected rizero/Kst =   0.747615194835508     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5003
 Corrected rizero/Kst =   0.820714868967252     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5004
 Corrected rizero/Kst =   0.798481699666072     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5005
 Corrected rizero/Kst =   0.806482983676089     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5006
 Corrected rizero/Kst =   0.785703593231642     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5007
 Corrected rizero/Kst =   0.760463985026753     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5008
 Corrected rizero/Kst =   0.742210156007276     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5009
 Corrected rizero/Kst =   0.712574097125327     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5010
 Corrected rizero/Kst =   0.770547828591144     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5011
 Corrected rizero/Kst =   0.832050261309626     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5012
 Corrected rizero/Kst =   0.834754551560094     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5013
 Corrected rizero/Kst =   0.833241561197396     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5014
 Corrected rizero/Kst =   0.829275236084934     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5084
 Corrected rizero/Kst =   0.858549681454355     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5085
 Corrected rizero/Kst =   0.852599481606575     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5086
 Corrected rizero/Kst =   0.825022268138985     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5087
 Corrected rizero/Kst =   0.794351531002231     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5088
 Corrected rizero/Kst =   0.781817634972699     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5089
 Corrected rizero/Kst =   0.777301674791415     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5090
 Corrected rizero/Kst =   0.753291051651343     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5091
 Corrected rizero/Kst =   0.791176344044980     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5092
 Corrected rizero/Kst =   0.848257415365455     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5093
 Corrected rizero/Kst =   0.845210526798913     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5094
 Corrected rizero/Kst =   0.824163347416689     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5166
 Corrected rizero/Kst =   0.873498079889370     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5167
 Corrected rizero/Kst =   0.811187018736729     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5168
 Corrected rizero/Kst =   0.774988047251346     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5169
 Corrected rizero/Kst =   0.776232275846319     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5170
 Corrected rizero/Kst =   0.787412285977111     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5171
 Corrected rizero/Kst =   0.803812414510610     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5172
 Corrected rizero/Kst =   0.831804079615452     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5173
 Corrected rizero/Kst =   0.829690218123376     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5226
 Corrected rizero/Kst =   0.730144254744044     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5250
 Corrected rizero/Kst =   0.830294761579570     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5251
 Corrected rizero/Kst =   0.833448400677105     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5252
 Corrected rizero/Kst =   0.825390667695947     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         5986
 Corrected rizero/Kst =   0.871044793775369     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6269
 Corrected rizero/Kst =   0.865759111083759     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6270
 Corrected rizero/Kst =   0.748924018745162     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6338
 Corrected rizero/Kst =   0.796067486039522     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6350
 Corrected rizero/Kst =   0.608369751985987     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6351
 Corrected rizero/Kst =   0.735562627726998     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6352
 Corrected rizero/Kst =   0.822559923183863     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6353
 Corrected rizero/Kst =   0.726060958761219     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6354
 Corrected rizero/Kst =   0.759172469815581     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6405
 Corrected rizero/Kst =   0.789352995274669     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6406
 Corrected rizero/Kst =   0.773930837285717     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6409
 Corrected rizero/Kst =   0.668780186227450     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6410
 Corrected rizero/Kst =   0.727439777689404     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6416
 Corrected rizero/Kst =   0.485274039712658     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6417
 Corrected rizero/Kst =   0.561643577403172     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6418
 Corrected rizero/Kst =   0.509836179355826     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6419
 Corrected rizero/Kst =   0.497846814230143     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6420
 Corrected rizero/Kst =   0.644936019660394     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6421
 Corrected rizero/Kst =   0.645367148883507     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6422
 Corrected rizero/Kst =   0.636048437946625     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6423
 Corrected rizero/Kst =   0.687524868445467     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6478
 Corrected rizero/Kst =   0.724451627278066     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6479
 Corrected rizero/Kst =   0.785906204414923     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6480
 Corrected rizero/Kst =   0.704134187393615     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6481
 Corrected rizero/Kst =   0.704134187393615     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6482
 Corrected rizero/Kst =   0.760186577073150     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6483
 Corrected rizero/Kst =   0.574301757092971     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6484
 Corrected rizero/Kst =   0.426207658049096     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6485
 Corrected rizero/Kst =   0.488183351307945     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6486
 Corrected rizero/Kst =   0.488183351307945     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6487
 Corrected rizero/Kst =   0.412794117587252     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6488
 Corrected rizero/Kst =   0.440164043464598     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6489
 Corrected rizero/Kst =   0.496632217706388     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6490
 Corrected rizero/Kst =   0.613020111962395     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6491
 Corrected rizero/Kst =   0.700204193026489     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6543
 Corrected rizero/Kst =   0.691658265476872     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6544
 Corrected rizero/Kst =   0.696466561623081     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6545
 Corrected rizero/Kst =   0.766510256580689     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6546
 Corrected rizero/Kst =   0.808982102792546     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6547
 Corrected rizero/Kst =   0.744747303858899     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6548
 Corrected rizero/Kst =   0.797185681924534     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6549
 Corrected rizero/Kst =   0.902292105568026     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6550
 Corrected rizero/Kst =   0.860878098429688     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6551
 Corrected rizero/Kst =   0.612035772043885     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6552
 Corrected rizero/Kst =   0.542052461757367     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6553
 Corrected rizero/Kst =   0.544192488966847     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6554
 Corrected rizero/Kst =   0.509855247735395     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6555
 Corrected rizero/Kst =   0.506059330228411     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6556
 Corrected rizero/Kst =   0.502998501466848     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6557
 Corrected rizero/Kst =   0.605031498698972     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6558
 Corrected rizero/Kst =   0.655542244949184     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6606
 Corrected rizero/Kst =   0.615366814946893     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6607
 Corrected rizero/Kst =   0.643007367394041     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6608
 Corrected rizero/Kst =   0.670816301818129     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6609
 Corrected rizero/Kst =   0.714275788025751     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6610
 Corrected rizero/Kst =   0.753605140700151     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6611
 Corrected rizero/Kst =   0.751415347669289     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6612
 Corrected rizero/Kst =   0.712846008931767     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6613
 Corrected rizero/Kst =   0.689159448451971     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6614
 Corrected rizero/Kst =   0.784387868028250     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6618
 Corrected rizero/Kst =   0.820804903490779     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6619
 Corrected rizero/Kst =   0.715603240796162     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6620
 Corrected rizero/Kst =   0.758524109882129     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6621
 Corrected rizero/Kst =   0.676662273323112     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6622
 Corrected rizero/Kst =   0.580177791004931     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6623
 Corrected rizero/Kst =   0.683538909130503     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6624
 Corrected rizero/Kst =   0.783830674611881     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6668
 Corrected rizero/Kst =   0.687216323745126     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6669
 Corrected rizero/Kst =   0.731652861338151     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6670
 Corrected rizero/Kst =   0.641718034268449     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6671
 Corrected rizero/Kst =   0.544108730460156     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6672
 Corrected rizero/Kst =   0.600850137076636     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6673
 Corrected rizero/Kst =   0.668090363151477     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6674
 Corrected rizero/Kst =   0.684171418412460     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6675
 Corrected rizero/Kst =   0.654866111949180     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6676
 Corrected rizero/Kst =   0.594967545294179     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6677
 Corrected rizero/Kst =   0.574560198893960     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6678
 Corrected rizero/Kst =   0.589812566799942     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6679
 Corrected rizero/Kst =   0.705518631496831     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6680
 Corrected rizero/Kst =   0.788304751741913     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6686
 Corrected rizero/Kst =   0.786513208453435     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6687
 Corrected rizero/Kst =   0.613106153409695     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6688
 Corrected rizero/Kst =   0.597734830648940     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6731
 Corrected rizero/Kst =   0.690664826508496     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6732
 Corrected rizero/Kst =   0.692029271339780     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6733
 Corrected rizero/Kst =   0.747813256774532     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6734
 Corrected rizero/Kst =   0.678877238583155     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6735
 Corrected rizero/Kst =   0.544108730460156     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6736
 Corrected rizero/Kst =   0.598524399996832     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6737
 Corrected rizero/Kst =   0.703821195621412     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6738
 Corrected rizero/Kst =   0.697734558630953     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6739
 Corrected rizero/Kst =   0.654781426514084     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6740
 Corrected rizero/Kst =   0.663614466655460     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6741
 Corrected rizero/Kst =   0.650605355223330     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6742
 Corrected rizero/Kst =   0.711902613110657     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6743
 Corrected rizero/Kst =   0.937524560309165     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6744
 Corrected rizero/Kst =   0.956588072517150     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6794
 Corrected rizero/Kst =   0.680345258930733     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6795
 Corrected rizero/Kst =   0.668048545087178     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6796
 Corrected rizero/Kst =   0.755113279420783     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6797
 Corrected rizero/Kst =   0.754964166986281     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6798
 Corrected rizero/Kst =   0.619367882158131     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6799
 Corrected rizero/Kst =   0.610906787784837     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6800
 Corrected rizero/Kst =   0.641612683228893     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6801
 Corrected rizero/Kst =   0.641437294425512     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6802
 Corrected rizero/Kst =   0.613073337177040     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6803
 Corrected rizero/Kst =   0.641612683228893     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6804
 Corrected rizero/Kst =   0.650605355223330     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6805
 Corrected rizero/Kst =   0.732469219224837     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6806
 Corrected rizero/Kst =   0.827360151511081     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6807
 Corrected rizero/Kst =   0.854638304137164     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6808
 Corrected rizero/Kst =   0.841495686680659     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6856
 Corrected rizero/Kst =   0.680239978899563     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6857
 Corrected rizero/Kst =   0.654040408467810     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6858
 Corrected rizero/Kst =   0.641437294425512     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6859
 Corrected rizero/Kst =   0.689758292991897     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6860
 Corrected rizero/Kst =   0.687942739673802     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6861
 Corrected rizero/Kst =   0.641291468591207     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6862
 Corrected rizero/Kst =   0.622785576076220     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6863
 Corrected rizero/Kst =   0.567366805499324     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6864
 Corrected rizero/Kst =   0.567623033976884     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6865
 Corrected rizero/Kst =   0.561797214565634     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6866
 Corrected rizero/Kst =   0.524985518581398     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6867
 Corrected rizero/Kst =   0.548592388293773     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6868
 Corrected rizero/Kst =   0.611223857651195     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6869
 Corrected rizero/Kst =   0.664548392933647     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6870
 Corrected rizero/Kst =   0.732163416256523     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6871
 Corrected rizero/Kst =   0.801605687902477     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6872
 Corrected rizero/Kst =   0.712989206206763     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6922
 Corrected rizero/Kst =   0.632419544475234     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6923
 Corrected rizero/Kst =   0.655776026770073     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6924
 Corrected rizero/Kst =   0.686537444260251     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6925
 Corrected rizero/Kst =   0.639127479899966     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6926
 Corrected rizero/Kst =   0.581638780776192     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6927
 Corrected rizero/Kst =   0.574792590443046     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6928
 Corrected rizero/Kst =   0.548897335514459     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6929
 Corrected rizero/Kst =   0.556074831206833     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6930
 Corrected rizero/Kst =   0.642149351891643     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6931
 Corrected rizero/Kst =   0.706072299701002     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6932
 Corrected rizero/Kst =   0.721661752623218     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6933
 Corrected rizero/Kst =   0.768221279425019     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6934
 Corrected rizero/Kst =   0.672398183426576     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6985
 Corrected rizero/Kst =   0.740341553571469     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6986
 Corrected rizero/Kst =   0.721387193542363     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6987
 Corrected rizero/Kst =   0.752414090973690     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6988
 Corrected rizero/Kst =   0.718345603401391     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6989
 Corrected rizero/Kst =   0.646302976590842     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6990
 Corrected rizero/Kst =   0.641437294425512     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6991
 Corrected rizero/Kst =   0.665436597150604     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6992
 Corrected rizero/Kst =   0.681947538890222     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6993
 Corrected rizero/Kst =   0.801783665024787     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6994
 Corrected rizero/Kst =   0.857142841600759     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6995
 Corrected rizero/Kst =   0.801783665024787     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6996
 Corrected rizero/Kst =   0.742781383144161     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         6997
 Corrected rizero/Kst =   0.561336244977670     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7045
 Corrected rizero/Kst =   0.808361766476948     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7046
 Corrected rizero/Kst =   0.762477054621063     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7047
 Corrected rizero/Kst =   0.792919738854581     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7048
 Corrected rizero/Kst =   0.802837235717831     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7049
 Corrected rizero/Kst =   0.708023995417730     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7050
 Corrected rizero/Kst =   0.668048545087178     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7051
 Corrected rizero/Kst =   0.680345258930733     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7052
 Corrected rizero/Kst =   0.729222807734453     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7053
 Corrected rizero/Kst =   0.830057343886535     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7054
 Corrected rizero/Kst =   0.835066843830820     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7055
 Corrected rizero/Kst =   0.801783665024787     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7056
 Corrected rizero/Kst =   0.830057343886535     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7057
 Corrected rizero/Kst =   0.790397873519917     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7105
 Corrected rizero/Kst =   0.762280303217211     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7106
 Corrected rizero/Kst =   0.762280303217211     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7214
 Corrected rizero/Kst =   0.514495782742011     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7215
 Corrected rizero/Kst =   0.677199125996425     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7216
 Corrected rizero/Kst =   0.893775828888649     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7217
 Corrected rizero/Kst =   0.874806550380753     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7218
 Corrected rizero/Kst =   0.808007869170284     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7219
 Corrected rizero/Kst =   0.754754336429038     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7272
 Corrected rizero/Kst =   0.501690388095823     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7273
 Corrected rizero/Kst =   0.561643577403172     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7274
 Corrected rizero/Kst =   0.800861400754627     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7275
 Corrected rizero/Kst =   0.844698332544705     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7276
 Corrected rizero/Kst =   0.750505661474881     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7277
 Corrected rizero/Kst =   0.713603270671475     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7565
 Corrected rizero/Kst =   0.865122439317888     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7566
 Corrected rizero/Kst =   0.798228089753500     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7567
 Corrected rizero/Kst =   0.552344701000992     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7621
 Corrected rizero/Kst =   0.768221279425019     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7622
 Corrected rizero/Kst =   0.617213428069695     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7676
 Corrected rizero/Kst =   0.748539454608845     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7677
 Corrected rizero/Kst =   0.772987964073776     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate, cell         7731
 Corrected rizero/Kst =   0.899438048702574     
 Original rizero, kst  1.000000000000000E-009  1.000000000000000E-013
 Set pore presssures to zero
 Adjusted steady infiltration rate at          288  cells
 The final true erosion volume is    1289102.55092472     
 The final true deposition volume is    902008.113166876     
 tempoutflowvolume    3222.92310877044       totaloutflowvolume 
   3222.92310877044     
 ==================================================================
 Total flow volume is    877981.908254402     
 Total deposit volume is    924836.380888588     
 Total volume is    1802818.28914299     
 ==================================================================
 Mass balance  inflow - outflow volume
 *** Inflow (Cubic Meters) ***
                                                Water
 Rainfall volume                                   1958646.04415904     
 Inflow Hydrograph                                0.000000000000000E+000
 Erosion volume                                    1182267.11366523     
 Inflow Hydrograph + Rainfall                      3140913.15782427     
 *** Outflow (Cubic Meters) ***
                                                Water
 Water lost to infiltration & interception         1464535.65055642     
 Floodplain storage                                877981.908254402     
 Floodplain deposite                               924836.380888588     
 Floodplain outflow hydrograph                     3222.92310877044     
 FLoodplain outflow, infiltration & storage        3270576.86280818     
 ==================================================================
 Volume error is   -129663.704983911       Volume relative error is 
 -4.128216810480999E-002
 The total number of times is       180866
 The average time step interval is            0
